# 

1 Which of the following protocols use distance-vector routing?

1. *RIP*
2. BGP
3. OSPF
4. DHCP

2 Which of the following devices is responsible for selecting the best path for a datagram?

1. Switch
2. NIC
3. Hub
4. *Router*