# 

1 Which of the following protocols use distance-vector routing?

1. *RIP*
2. DHCP
3. BGP
4. OSPF

2 Which of the following devices is responsible for selecting the best path for a datagram?

1. Switch
2. Hub
3. NIC
4. *Router*