# 

1 Which of the following protocols use distance-vector routing?

1. OSPF
2. *RIP*
3. DHCP
4. BGP

2 Which of the following devices is responsible for selecting the best path for a datagram?

1. NIC
2. *Router*
3. Hub
4. Switch